**Kompatybilność chłodzeń Frost, Frost Black oraz Vortex z LGA 1200/1700**Zdarza się, że producenci w niektórych nowych modelach płyt głównych montują podzespoły pozostawiając wyjątkowo mało miejsca pomiędzy komponentami. W takiej sytuacji może występować utrudniony montaż chłodzeń.  
Aby poprawnie zamontować układ chłodzenia Savio należy:  
1) Zdemontować wentylator przymocowany do radiatora. Pozwoli to na szybszy i łatwiejszy proces montażowy.  
2) Użyć kwadratowego koszyka montażowego (dla płyt głównych wymienionych poniżej).  
3) Radiator skierować większą klamrą ramki montażowej ku górze obudowy (dla chłodzenia VORTEX).  
  
**Lista płyt głównych, w których może wystąpić utrudniony montaż  
ASUS**  
ROG STRIX Z590-I GAMING WIFI  
ROG STRIX Z590-A GAMING WIFI  
ROG STRIX Z590-F GAMING WIFI  
PRIME Z590-A  
ProArt Z690-CREATOR WIFI  
ProArt B660-CREATOR D4  
ROG STRIX B660-G GAMING WIFI  
ROG STRIX B660-I GAMING WIFI  
ROG STRIX B660-A GAMING WIFI DDR4  
ROG MAXIMUS Z690 EXTREME GLACIAL  
ROG STRIX Z690-A GAMING WIFI  
ROG STRIX Z690-F GAMING WIFI   
TUF GAMING H670-PRO WIFI DDR4  
ROG STRIX Z690-I GAMING WIFI   
ROG STRIX Z690-E GAMING WIFI   
PRIME Z690-A DDR5  
TUF GAMING B560-PLUS WIFI  
Z690 STEEL LEGEND DDR5  
**ASROCK**H470 Steel Legend   
Z590 Taichi  
Z590 Steel Legend  
**GIGABYTE**  
B660M Gaming  
Z490I AROUS ULTRA  
ROG STRIX Z490-I GAMING   
Z490-G GAMING WI-FI  
B560 AORUS PRO AX  
B560I AORUS PRO AX  
Z590 AORUS ELITE AX  
Z590 AORUS ELITE   
Z590I AORUS ULTRA

Z590I VISION D  
Z590 Gaming X  
Z590M Gaming X  
B660 AORUS MASTER  
B660M AORUS PRO DDR4  
B660M AORUS PRO AX DDR4  
B660I AORUS PRO DDR4  
B660 GAMING X DDR4  
B660 GAMING X AX DDR4  
B660M GAMING X AX DDR4  
Z690 AORUS ULTRA   
Z690I AORUS ULTRA   
Z690 AORUS PRO  
Z690M A ELITE AX   
Z690 AERO G DDR5  
Z690 AERO G DDR4  
Z690 AORUS ELITE  
Z690 AORUS ELITE DDR4  
Z690 AORUS ELITE AX DDR4  
Z690 GAMING X DDR4  
Z690 UD DDR4  
Z690 UD  
Z690 UD AX DDR4  
Z690 UD AC  
Z690 UD AX  
Z690 UD AX DDR5  
Z690 AORUS PRO DDR5  
Z590I VISION D