**Kompatybilność chłodzeń Frost, Frost Black oraz Vortex z LGA 1200/1700**Zdarza się, że producenci w niektórych nowych modelach płyt głównych montują podzespoły pozostawiając wyjątkowo mało miejsca pomiędzy komponentami. W takiej sytuacji może występować utrudniony montaż chłodzeń.
Aby poprawnie zamontować układ chłodzenia Savio należy:
1) Zdemontować wentylator przymocowany do radiatora. Pozwoli to na szybszy i łatwiejszy proces montażowy.
2) Użyć kwadratowego koszyka montażowego (dla płyt głównych wymienionych poniżej).
3) Radiator skierować większą klamrą ramki montażowej ku górze obudowy (dla chłodzenia VORTEX).

**Lista płyt głównych, w których może wystąpić utrudniony montaż
ASUS**
ROG STRIX Z590-I GAMING WIFI
ROG STRIX Z590-A GAMING WIFI
ROG STRIX Z590-F GAMING WIFI
PRIME Z590-A
ProArt Z690-CREATOR WIFI
ProArt B660-CREATOR D4
ROG STRIX B660-G GAMING WIFI
ROG STRIX B660-I GAMING WIFI
ROG STRIX B660-A GAMING WIFI DDR4
ROG MAXIMUS Z690 EXTREME GLACIAL
ROG STRIX Z690-A GAMING WIFI
ROG STRIX Z690-F GAMING WIFI
TUF GAMING H670-PRO WIFI DDR4
ROG STRIX Z690-I GAMING WIFI
ROG STRIX Z690-E GAMING WIFI
PRIME Z690-A DDR5
TUF GAMING B560-PLUS WIFI
Z690 STEEL LEGEND DDR5
**ASROCK**H470 Steel Legend
Z590 Taichi
Z590 Steel Legend
**GIGABYTE**
B660M Gaming
Z490I AROUS ULTRA
ROG STRIX Z490-I GAMING
Z490-G GAMING WI-FI
B560 AORUS PRO AX
B560I AORUS PRO AX
Z590 AORUS ELITE AX
Z590 AORUS ELITE
Z590I AORUS ULTRA

Z590I VISION D
Z590 Gaming X
Z590M Gaming X
B660 AORUS MASTER
B660M AORUS PRO DDR4
B660M AORUS PRO AX DDR4
B660I AORUS PRO DDR4
B660 GAMING X DDR4
B660 GAMING X AX DDR4
B660M GAMING X AX DDR4
Z690 AORUS ULTRA
Z690I AORUS ULTRA
Z690 AORUS PRO
Z690M A ELITE AX
Z690 AERO G DDR5
Z690 AERO G DDR4
Z690 AORUS ELITE
Z690 AORUS ELITE DDR4
Z690 AORUS ELITE AX DDR4
Z690 GAMING X DDR4
Z690 UD DDR4
Z690 UD
Z690 UD AX DDR4
Z690 UD AC
Z690 UD AX
Z690 UD AX DDR5
Z690 AORUS PRO DDR5
Z590I VISION D